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AIRCRAFT MAINTENANCE PROGRAMME (AMP) COMPLIANCE CHECKLIST
In accordance with Part-M, M.A.302 AMC and Appendix I to AMC M.A.302 and AMC M.B.301(b) — Content of the maintenance programme
Section 1 – AMP & Applicant’s Details 
	CAMO Name
	
	CAMO Approval No.
	

	CAME Reference
	
	AOC Approval No. (if applicable)
	

	Applicant’s Name
	
	Brunei DCA AMP Reference
	

	Applicant’s Contact E-mail
	
	CAMO AMP Reference 
	

	Applicant’s Signature & Date
	


	AMP Issue/ Revision/Date 
	

	Review by:
(Brunei DCA Use Only)
	Previous AMP (if applicable)
	

	Inspector’s Name
	
	Aircraft & Engine Type
	

	Inspector’s Signature & Date
	



	Aircraft Registrations
	





Section 2 – Instructions for completion 
The purpose of the Aircraft Maintenance Programme Compliance Checklist is to assist owners/ operators with a view to ensure that the Aircraft Maintenance Programmes submitted to the Brunei DCA for approval are standardised and include all items that are required by BAR 8 Part M.A.302, AMC M.A.302 and also other additional Brunei DCA national requirements, not limiting to BAR 8 Part-26. This checklist, when completed, should be submitted with the draft aircraft maintenance programme. 

This document shall be accompanied with a completed AIR Form 981 – Application for the approval of Aircraft Maintenance Programme and AIR H012 – Aircraft Maintenance Programme Preface Documents. The maintenance programme shall includes all the relevant information as detailed in Appendix I to AMC M.A.302 and AMC M.B.301(b) — Content of the maintenance programme, the format of which may be modified to suit the operator's preferred method. In all cases the checklist should clearly show either compliance (‘yes’) & location of the compliance in the notes section or not applicable (‘no’) & the reason in the notes section.

The specific tasks and the relevant control procedures shall be included as specified in the Aircraft Maintenance Programme (AMP) or Continuing Airworthiness Management Exposition (CAME) of the operator / CAMO managing the aircraft. The relevant cross-references shall be specified in the compliance note’s column at the appropriate paragraphs and the correct term AMP or CAME shall be used. 

The checklist is provided to ensure the minimum required items are contained in the Maintenance Programme. It should be enhanced as necessary to suit the aircraft's needs; operational, utilisation & environmental.

Once completed please return this document to the Brunei DCA via e-mail address airworth.regulatory@dca.gov.bn , copy to: regulatory.dca@dca.gov.bn and/or dispatch to the following address:

Airworthiness Section
Regulatory Division
Department of Civil Aviation
Ministry of Transport and Infocommunications
Brunei International Airport
Bandar Seri Begawan
BB2513
Negara Brunei Darussalam



Section 3 – AMP Compliance Checklists 
	Item
	Description
	Compliance
	Compliance Notes
	Remarks
(Brunei DCA Use Only)

	
	
	Yes
	No
	
	

	1. GENERAL REQUIREMENTS

	1.1
	Maintenance Programme Basic Information (Introduction/ Administration)

	1.1.1
	The type/model/ and registration number of the aircraft
	|_|
	|_|
	
	

	
	The type/model of the engines
	|_|
	|_|
	
	

	
	The type/model of the propellers, where applicable
	|_|
	|_|
	
	

	
	The type/model of the auxiliary power units, where applicable
	|_|
	|_|
	
	

	1.1.2
	The name and address of the owner, operator, CAMO organisation managing the aircraft airworthiness
	|_|
	|_|
	
	

	1.1.3
	The programme reference, the date of issue and issue number
	|_|
	|_|
	
	

	1.1.4
	A signed statement. See AIR H012 for the suitable statement
	|_|
	|_|
	
	

	1.1.5
	Contents list
	|_|
	|_|
	
	

	
	List of effective pages
	|_|
	|_|
	
	

	
	Revision status of the document
	|_|
	|_|
	
	

	1.1.6
	Check periods for anticipated utilisation; include a utilisation tolerance of not more than 25%. Where utilisation cannot be anticipated, calendar time limits should also be included
	|_|
	|_|
	
	

	1.1.7
	Procedures for escalation where applicable & acceptable to the Brunei DCA
	|_|
	|_|
	
	

	1.1.8
	Date and reference of approved amendments
	|_|
	|_|
	
	

	1.1.9
	Pre-flight maintenance tasks that are accomplished by maintenance staff
	|_|
	|_|
	
	

	1.1.10
	The tasks and the periods (intervals / frequencies) at which inspections should be carried out, including the task effectivity and type and degree of inspection of the:

	
	a. Aircraft
	|_|
	|_|
	
	

	
	b. Engine(s)
	|_|
	|_|
	
	

	
	c. APU
	|_|
	|_|
	
	

	
	d. Propeller(s)
	|_|
	|_|
	
	

	
	e. Components
	|_|
	|_|
	
	

	
	f.  Accessories
	|_|
	|_|
	
	

	
	g. Equipment
	|_|
	|_|
	
	

	
	h. Instruments
	|_|
	|_|
	
	

	
	i.  Electrical and radio apparatus
	|_|
	|_|
	
	

	1.1.11
	The periods at which components should be:

	
	a. Checked
	|_|
	|_|
	
	

	
	b. Cleaned
	|_|
	|_|
	
	

	
	c. Lubricated
	|_|
	|_|
	
	

	
	d. Replenished
	|_|
	|_|
	
	

	
	e. Adjusted
	|_|
	|_|
	
	

	
	f.  Tested
	|_|
	|_|
	
	

	1.1.12
	Details of ageing aircraft system requirements with any specified sampling programmes, (if applicable)
	|_|
	|_|
	
	

	1.1.13
	Details of specific structural maintenance programmes, (if applicable), including but not limited to:

	
	a. Damage Tolerance and Supplemental Structural Inspection Programmes (SSID)
	|_|
	|_|
	
	

	
	b. SB review performed by the TC holder
	|_|
	|_|
	
	

	
	c. Corrosion prevention and control
	|_|
	|_|
	
	

	
	d. Repair Assessment
	|_|
	|_|
	
	

	
	e. Widespread Fatigue Damage
	|_|
	|_|
	
	

	1.1.14
	If applicable, details of Critical Design Configuration Control Limitations together with appropriate procedures.
	|_|
	|_|
	
	

	1.1.15
	Statement of the limit of validity for the structural programme in 1.1.13, if applicable
	|_|
	|_|
	
	

	1.1.16
	The periods at which overhauls should be made
	|_|
	|_|
	
	

	
	The periods at which replacements should be made
	|_|
	|_|
	
	

	1.1.17
	A cross-reference to other documents related to:

	
	a. Mandatory life limitations
	|_|
	|_|
	
	

	
	b. Certification Maintenance Requirements (CMR's), (if applicable)
	|_|
	|_|
	
	

	
	c. Airworthiness Directives (AD)
	|_|
	|_|
	
	

	
	Specific identification of the above items mandatory status
	|_|
	|_|
	
	

	1.1.18
	Reliability programme or statistical methods of continuous Surveillance (CMPA MA.302(g))
	|_|
	|_|
	
	

	1.1.19
	A statement that practices and procedures should be the standards specified by the TC holder
	|_|
	|_|
	
	

	1.1.20
	Each maintenance task (i.e. inspections - detailed, scan, general) should be defined in a definition section
	|_|
	|_|
	
	

	2. PROGRAMME BASIS

	2.1
	Is the programme based upon the MRB report, the TC holder's maintenance planning document or Chapter 5 of the maintenance manual?
	|_|
	|_|
	
	

	2.2
	For newly type-certificated aircraft / comprehensively appraise the manufacturer's recommendations (and MRB report where applicable)
	|_|
	|_|
	
	

	2.3
	For existing aircraft types, comparisons with maintenance programmes previously approved
	|_|
	|_|
	
	

	2.4
	If CDCCL have been identified by the TC/STC holder, have maintenance instructions been developed
	|_|
	|_|
	
	

	3. AMENDMENTS PROCEDURES

	3.1
	Amendments (revisions) to reflect changes: 
(See AIR H012 for the Aircraft Maintenance Programme Amendment Approval Submission)
	|_|
	|_|
	
	

	
	a. In the TC holder's recommendations
	|_|
	|_|
	
	

	
	b. Introduced by modifications
	|_|
	|_|
	
	

	
	c. Discovered by service experience
	|_|
	|_|
	
	

	
	d. As required by the Brunei DCA
	|_|
	|_|
	
	

	4. PERMITTED VARIATIONS TO MAINTENANCE PERIODS (with the exception of items identified in 1.1.16)

	4.1
	Process in place to vary the periods through a Procedure approved by the Brunei DCA? (Refer to AIR H012 Permitted Variations)
	|_|
	|_|
	
	

	
	Vary the periods with the approval by the Brunei DCA (including temporary amendments to maintenance programme, if required)
	|_|
	|_|
	
	

	5. PERIODIC REVIEW OF MAINTENANCE PROGRAMME CONTENTS

	5.1
	Periodic review to ensure that the programme reflects current:

	
	a. TC holder's recommendations
	|_|
	|_|
	
	

	
	b. Revisions to the MRB report (if applicable)
	|_|
	|_|
	
	

	
	c. Mandatory requirements
	|_|
	|_|
	
	

	
	d. Maintenance needs of the aircraft
	|_|
	|_|
	
	

	5.2
	Annual review defined
	|_|
	|_|
	
	

	6. RELIABILITY PROGRAMMES

	6.1
	Applicability

	6.1.1
	Developed in the following cases:
	|_|
	|_|
	
	

	
	a. Programme is based upon MSG-3 logic
	|_|
	|_|
	
	

	
	b. Programme includes condition monitored components
	|_|
	|_|
	
	

	
	c. Programme does not contain overhaul time periods for all significant system components
	|_|
	|_|
	
	

	
	d. Specified by the Manufacturer's MPD or MRB
	|_|
	|_|
	
	

	6.1.2
	Need not be developed in the following cases:

	
	a. Programme is based upon the MSG-1 or 2 logic (only hard times or on condition items)
	|_|
	|_|
	
	

	
	b. Not a complex motor powered aircraft (CMPA)
	|_|
	|_|
	
	

	
	c. Programme provides overhaul time periods for all significant system components
	|_|
	|_|
	
	

	6.1.3
	Operator may develop own reliability monitoring programme
	|_|
	|_|
	
	

	6.2
	Applicability, small fleets

	6.2.1
	Less than 6 aircraft of the same type
	|_|
	|_|
	
	

	6.2.2
	Reliability programme is irrespective of the fleet size
	|_|
	|_|
	
	

	6.2.3
	Tailor reliability programmes to suit the size and complexity of operation
	|_|
	|_|
	
	

	6.2.4
	Use of "Alert levels" should be used carefully
	|_|
	|_|
	
	

	6.2.5
	When establishing a reliability programme, consider the following:

	
	a. Focus on areas where a sufficient amount of data is likely to be processed
	|_|
	|_|
	
	

	
	b. How is engineering judgment applied?
	|_|
	|_|
	
	

	6.2.6
	Pool data and analysis (paragraph 6.6 specifies conditions)
	|_|
	|_|
	
	

	6.2.7
	If unable to pool data / additional restrictions on the MRB/MPD tasks intervals specified
	|_|
	|_|
	
	

	6.3
	Engineering judgement

	6.3.1
	Are there appropriately qualified personnel (with appropriate engineering experience and understanding of reliability concept) for the reliability programme?
	|_|
	|_|
	
	

	6.4
	Contracted Maintenance
	
	
	
	

	6.4.1
	Maintenance programme / may sub-contract certain functions to the Part-145 organisation
	|_|
	|_|
	
	

	6.4.2
	These are:

	
	a. Developing the maintenance and reliability programmes
	|_|
	|_|
	
	

	
	b. Collection and analysis of the reliability data
	|_|
	|_|
	
	

	
	c. Providing reliability reports
	|_|
	|_|
	
	

	
	d. Proposing corrective actions
	|_|
	|_|
	
	

	6.4.3
	Approval to implement a corrective action / CAMO prerogative and responsibility
	|_|
	|_|
	
	

	6.4.4
	Maintenance contract / CAME, and MOE procedures
	|_|
	|_|
	
	

	6.5
	Reliability programme

	6.5.1.
	Objectives:

	6.5.1.1
	Statement summarising the prime objectives of the programme
	|_|
	|_|
	
	

	
	a. Recognise the need for corrective action
	|_|
	|_|
	
	

	
	b. Establish what corrective action is needed
	|_|
	|_|
	
	

	
	c. Determine the effectiveness of that action
	|_|
	|_|
	
	

	6.5.1.2
	The extent of the objectives should be directly related to the scope of the programme
	|_|
	|_|
	
	

	6.5.1.3
	All MSG-3 related tasks are effective and their periodicity is adequate
	|_|
	|_|
	
	

	6.5.2
	Identification of items:

	
	The items controlled by the programme should be stated
	|_|
	|_|
	
	

	6.5.3
	Terms and definitions:

	
	Significant terms and definitions should be clearly identified
	|_|
	|_|
	
	

	6.5.4
	Information sources and collection: 

	6.5.4.1
	Sources and procedures in the Exposition
	|_|
	|_|
	
	

	6.5.4.2
	Type of information to be collected should be related to the objectives, examples of the normal prime sources:

	
	a. Pilots Reports
	|_|
	|_|
	
	

	
	b. Technical Logs
	|_|
	|_|
	
	

	
	c. Aircraft Access Terminal / On-board readouts
	|_|
	|_|
	
	

	
	d. Maintenance Worksheets
	|_|
	|_|
	
	

	
	e. Workshop Reports
	|_|
	|_|
	
	

	
	f. Reports on Functional Checks
	|_|
	|_|
	
	

	
	g. Reports on Special Inspections
	|_|
	|_|
	
	

	
	h. Stores Issues/Reports
	|_|
	|_|
	
	

	
	i.  Air Safety Reports
	|_|
	|_|
	
	

	
	j.  Reports on Delays and Incidents
	|_|
	|_|
	
	

	
	k. Other sources: i.e. ETOPS, RVSM, CAT II/III
	|_|
	|_|
	
	

	6.5.4.3
	Due account  of continuing airworthiness and safety information promulgated appropriately approved i.a.w BAR 8 Part-21
	|_|
	|_|
	
	

	6.5.5
	Display of information:

	
	Information displayed graphically or tabular or a combination
	|_|
	|_|
	
	

	6.5.5.1
	Provisions for “nil returns”
	|_|
	|_|
	
	

	6.5.5.2
	Where “standards” or “alert levels”, information oriented accordingly
	|_|
	|_|
	
	

	6.5.6
	Examination, analysis and interpretation of the information:

	
	Method for examining, analysing and interpreting the information should be explained
	|_|
	|_|
	
	

	6.5.6.1
	Methods of examination may be varied - content & quantity
	|_|
	|_|
	
	

	6.5.6.2
	The whole process should enable a critical assessment of the effectiveness of the programme as a total activity. May involve:

	
	a. Comparisons of operational reliability with established or allocated standards
	|_|
	|_|
	
	

	
	b. Analysis and interpretation of trends
	|_|
	|_|
	
	

	
	c. Evaluation of repetitive defects
	|_|
	|_|
	
	

	
	d. Confidence testing of expected and achieved results
	|_|
	|_|
	
	

	
	e. Studies of life-bands and survival characteristics
	|_|
	|_|
	
	

	
	f. Reliability predictions
	|_|
	|_|
	
	

	6.5.6.3
	Range and depth of analysis should be related to the particular programme:

	
	a. Flight defects and reductions in reliability
	|_|
	|_|
	
	

	
	b. Defects – line and main base
	|_|
	|_|
	
	

	
	c. Deterioration observed – routine maintenance
	|_|
	|_|
	
	

	
	d. Workshop and overhaul findings
	|_|
	|_|
	
	

	
	e. Modification evaluations
	|_|
	|_|
	
	

	
	f. Sampling programmes
	|_|
	|_|
	
	

	
	g. Adequacy of maintenance equipment and publications
	|_|
	|_|
	
	

	
	h. Effectiveness of maintenance procedures
	|_|
	|_|
	
	

	
	i.  Staff training
	|_|
	|_|
	
	

	
	j. Service bulletins, technical instructions, etc.
	|_|
	|_|
	
	

	6.5.6.4
	Contracted maintenance - arrangements established and details for information input included
	|_|
	|_|
	
	

	6.5.7
	Corrective Actions

	6.5.7.1
	Procedures / time scales for implementing corrective actions / monitoring – should be fully described & could include:

	
	a. Changes to maintenance, operational procedures or techniques
	|_|
	|_|
	
	

	
	b. Changes requiring amendment of the approved maintenance programme?
	|_|
	|_|
	
	

	
	c. Amendments to approved manuals
	|_|
	|_|
	
	

	
	d. Initiation of modifications
	|_|
	|_|
	
	

	
	e. Special inspections / fleet campaigns
	|_|
	|_|
	
	

	
	f. Spares provisioning
	|_|
	|_|
	
	

	
	g. Staff training
	|_|
	|_|
	
	

	
	h. Manpower and equipment planning
	|_|
	|_|
	
	

	6.5.7.2
	Procedures for effecting changes should be described
	|_|
	|_|
	
	

	6.5.8
	Organisational Responsibilities:

	
	Organisational structure – chains of responsibility should be defined
	|_|
	|_|
	
	

	6.5.9
	Presentation of information to the Brunei DCA

	
	Information submitted to the Brunei DCA for approval of the reliability programme:

	
	a. Format and content of routine reports
	|_|
	|_|
	
	

	
	b. Time scales for reports / distribution
	|_|
	|_|
	
	

	
	c. Format and content of reports requesting amendments
	|_|
	|_|
	
	

	6.5.10
	Evaluation and review:

	
	Describe procedures and individual responsibilities - continuous monitoring of the effectiveness of the programme
	|_|
	|_|
	
	

	6.5.10.1
	Procedures for revising the "standards" or "alert levels"
	|_|
	|_|
	
	

	6.5.10.2
	Criteria to be taken into account during the review includes:

	
	a. Utilisation (high / low / seasonal)
	|_|
	|_|
	
	

	
	b. Fleet commonality
	|_|
	|_|
	
	

	
	c. Alert Level adjustment criteria
	|_|
	|_|
	
	

	
	d. Adequacy of data
	|_|
	|_|
	
	

	
	e. Reliability procedure audit
	|_|
	|_|
	
	

	
	f.  Staff training
	|_|
	|_|
	
	

	
	g. Operational and maintenance procedures
	|_|
	|_|
	
	

	6.5.11
	Approval of organisation to implement maintenance programme changes arising from the reliability programme results:

	
	a. Does the reliability programme monitor the content of the maintenance programme in a comprehensive manner?
	|_|
	|_|
	
	

	
	b. Is appropriate control exercised by the owner / operator over the internal validation of such changes?
	|_|
	|_|
	
	

	6.6
	Pooling Arrangements

	6.6.1
	Pooling information – must be substantially the same, including:

	
	a. Certification / modification / SB compliance
	|_|
	|_|
	
	

	
	b. Operational Factors
	|_|
	|_|
	
	

	
	c. Maintenance factors
	|_|
	|_|
	
	

	6.6.2
	Is there a substantial amount of commonality
/ has the Brunei DCA agreed?
	|_|
	|_|
	
	

	6.6.3
	Is the aircraft on short-term lease? Brunei DCA may grant more flexibility
	|_|
	|_|
	
	

	6.6.4
	Changes to any CAMO requires assessment in order that the pooling benefits can be maintained
	|_|
	|_|
	
	

	6.6.5
	Reliability programme managed by the aircraft manufacturer if agreed by the Brunei DCA
	|_|
	|_|
	
	

	7. BRUNEI DCA REQUIRED ITEMS (M.A.302(d))

	7.1
	Details of who may issue a CRS
	|_|
	|_|
	
	

	7.2
	Define which inspections/checks are considered to be base maintenance
	|_|
	|_|
	
	

	7.3
	Brunei DCA maintenance requirements, as adopted from best practices (UK CAP), in the absence of specific recommendations. 
See AIR H012 for details on the items below. 

	7.3.1
	Aircraft battery capacity check/deep cycle?
	|_|
	|_|
	
	

	7.3.2
	Emergency equipment
	|_|
	|_|
	
	

	7.3.3
	Emergency escape provisions:
	|_|
	|_|
	
	

	
	a. Portable valise type life-rafts
	|_|
	|_|
	
	

	
	b. Door & escape chutes/slides
	|_|
	|_|
	
	

	
	c. Emergency exits / hatches
	|_|
	|_|
	
	

	7.3.4
	Flexible hoses
	|_|
	|_|
	
	

	7.3.5
	Fuel / oil system contamination checks
	|_|
	|_|
	
	

	7.3.6
	Pressure vessels
	|_|
	|_|
	
	

	7.3.7
	Seat belts and harnesses
	|_|
	|_|
	
	

	7.3.8
	Vital points and control systems 
	|_|
	|_|
	
	

	7.3.9
	Altimeter & Speed Indicator
	|_|
	|_|
	
	

	7.3.10
	Compass Swing
	|_|
	|_|
	
	

	7.3.11
	Maintenance applicable to specific operations approvals, if applicable:

	
	LVO
	|_|
	|_|
	
	

	
	MNPS
	|_|
	|_|
	
	

	
	RVSM
	|_|
	|_|
	
	

	
	ETOPS
	|_|
	|_|
	
	

	
	CAT.POL.H.305
	Helicopter Ops without an assured safe forced landing capability
	|_|
	|_|
	
	

	
	SPA.HOFO.105
	Approval for offshore operations
	|_|
	|_|
	
	

	
	SPA.HOFO.155
	VHM system
	|_|
	|_|
	
	

	
	SPA.HHO.100
	Helicopter hoist operations (HHO)
	|_|
	|_|
	
	

	
	CAT.POL.H.420
	Helicopter Ops over a hostile environment
	|_|
	|_|
	
	

	
	SPA.HEMS.100
	Helicopter emergency medical service (HEMS) operations
	|_|
	|_|
	
	

	
	SPA.NVIS.100
	Night vision imaging system (NVIS) operations
	|_|
	|_|
	
	

	
	Part SPO. Subpart E
	Helicopter Ext Sling load Ops (HESLO)
	|_|
	|_|
	
	

	
	Transport of dangerous goods
	|_|
	|_|
	
	

	
	Other (Specify) …
	|_|
	|_|
	
	

	7.3.12
	Customer furnished equipment
	|_|
	|_|
	
	

	7.3.13
	Engine & APU condition monitored maintenance
	|_|
	|_|
	
	

	7.3.14
	General Requirement for Airworthiness i.a.w Volume I to the BAR 8 Part-26
	|_|
	|_|
	
	

	7.3.15
	Flight data recorder systems
	|_|
	|_|
	
	

	7.3.16
	Mode "S" transponder ICAO 24-bit aircraft addresses
	|_|
	|_|
	
	

	7.3.17
	In-flight entertainment systems (IFE)
	|_|
	|_|
	
	

	7.3.18
	Cockpit Voice Recorders
	|_|
	|_|
	
	

	7.3.19
	Identification of Critical Maintenance Tasks:

	
	Identification of all critical components within the maintenance programme
	|_|
	|_|
	
	

	
	Monitoring the health of all Critical components and premature failure
	|_|
	|_|
	
	

	
	Identification of Critical maintenance tasks including any calculation as part of a maintenance tasks that could adversely affect the safety or performance of the aircraft as per AMC1 M.A.402(h)
	|_|
	|_|
	
	


Section 4 – Applicant’s Declaration
	I, (………………insert applicant’s name………………) hereby certify that the above AMP compliance checklist is a correct reflection of the maintenance schedule and arrangements for the aircraft type/registrations above for the company (……….insert company name………….). I hereby certify that Human factors principles have also been observed throughout the design and organisation of the AMP.

Signed: …………………………………………………………………...                                    Date: ……………………………………
Position in company:……………………………………………………..
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